| **Hazards** | **Is the hazard present?****Y/N** | **What is the risk?** | **Risk rating****H = High****M = MediumL = Low** | **Control measures** | **Is this control in place?****Y/N** | **If no, what actions are required to implement the control?** | **Person responsible** | **Date action completed** |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Defective work equipment |  | Severe injuries arising from the use of defective work equipment | H | Maintain work equipment in a safe working orderCarry out inspections of work equipment to be used for work at height |  |  |  |  |
| Unsuitable working platforms |  | Severe injuries arising from the use of unsuitable elevated work platforms | H | The most suitable work equipment for working at height must be chosen 13Unsuitable elevated work platforms are not used for raising persons to a height |  |  |  |  |
| Accessing high windows |  | Falls from height | M | A window pole or step ladder is used to open windows at height that do not have opening mechanism at ground level |  |  |  |  |
| Use of ladders |  | Falls from height | H | [**See Cleaning (Work at Height – Ladders) – Template No. 9**](https://www.hsa.ie/eng/education/managing_safety_and_health_in_schools/new_guidelines_files/ms_word_files/cleaning-work-at-height-_ladders_%E2%80%93no-9.docx)[**Work at Height (General) - Template No. 15**](https://www.hsa.ie/eng/education/managing_safety_and_health_in_schools/new_guidelines_files/ms_word_files/work-at-height-_general_-no-15.docx) |  |  |  |  |

 13 This requirement arises out of Regulation 100 of the Safety, Health and Welfare at Work (General Application) Regulations 2007

© All Rights Reserved

If there is one or more **High Risk (H)** actions needed, then the risk of injury could be high and immediate action should be taken.

**Medium Risk (M)** actions should be dealt with as soon as possible. **Low Risk (L)** actions should be dealt with as soon as practicable.

Risk Assessment carried out by: Date: / /